

|  |  |  |  |
| --- | --- | --- | --- |
| **Part** | **Material** | **Part** | **Material** |
| Bearer | Glued 90X45 F7 H3 Treated Pine for 90X90 | Ledger | 90x45 F7 H3 Treated Pine |
| Bearer Stump | 90x300 Stirrup | Decking Board | 140x19x5700 Merbau Set Length |
| Bearer Footing | 200x200x400 Poured Concrete footing | Noggins | 90x45 F7 H3 Treated Pine |
| Joist | 90x45 F7 H3 Treated Pine | Deck Screws | 3m Gap Hidden fastener |
| Hanger | 45 Joist hanger | Joist Support | Klevaklip Adjustable Joist Support |